Rascal Requirements Verification Document

Saint Louis University

Rascal



Last Updated: 11/9/13

Document No: RCL-O-CMQA3

Copper Operational

Test Plan

|  |  |  |  |
| --- | --- | --- | --- |
| **Team Member** | **Position** | **Email** | **Phone** |
| Tom Moline | Program Manager/Navigation Engineer | [tmoline@slu.edu](mailto:tmoline@slu.edu) | 630-401-0791 |
| Nate Richard | Propulsion Team | [nrichar8@slu.edu](mailto:nrichar8@slu.edu) | 608-732-7147 |
| Tyler Olson | Structures Team | [tolson6@slu.edu](mailto:tolson6@slu.edu) | 812-204-1098 |
| Bryant Gaume | Propulsion Team | [gbryant1@slu.edu](mailto:gbryant1@slu.edu) | 636-448-0378 |
| Jennifer Babb | Propulsion Team | [jbabb1@slu.edu](mailto:jbabb1@slu.edu) | 636-579-6816 |

**Revisions Summary**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Revision** | **Description** | **Date** | **Prepared by** | **Approved by** |
| **-** | Description | 9/12/2013 | Insert Name Here | Insert Name Here |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

# INTRODUCTION

# NOMENCLATURE

Table of Contents

[INTRODUCTION 3](#_Toc371780710)

[NOMENCLATURE 4](#_Toc371780711)

[REQUIREMENT STAGES 6](#_Toc371780712)

[1. Pre-Launch Requirements 6](#_Toc371780713)

[2. Post-Launch Ejection Requirements 9](#_Toc371780714)

[3. Separation and Stabilization Requirements 10](#_Toc371780715)

[4. Stationkeeping Requirements 11](#_Toc371780716)

[5. “Escape” Requirements 12](#_Toc371780717)

[6. Rendezvous Requirements 13](#_Toc371780718)

# REQUIREMENT STAGES

# Pre-Launch Requirements

1. **The Total CubeSat System Volume Shall Not Exceed 6U**
2. **The Total CubeSat System Mass Shall Not Exceed 8.0 kg**
3. **All Materials Used in the CubeSat System shall have a Total Mass Loss of Less Than 1.0%**
4. **All Materials Used in the CubeSat System Shall Have a Collected Volatile Condensable Material of less than 0.1%**
5. **The CubeSat System Must be in Orbit for at Least 6 Months**
6. **The CubeSat System Must Deorbit within 25 Years of being Launched**
7. **Jade and Ruby Shall be Conjoined Prior to Launch Vehicle Integration**
8. **The CubeSat System Shall Incorporate a Deployment Switch**
9. **No Protrusion Shall Extend beyond 6.5 mm Normal to Any External Surface of Jade or Ruby**
10. **No External Components Other than the CubeSat Rails of Jade and Ruby may make Contact with the Deployer**
11. **The Deployer Shall not be Used to Secure Any CubeSat Deployables**
12. **The Center of Gravity of the total CubeSat System Shall be Located within a Sphere of 2 cm of the Geometric Center of the System**
13. **The Center of Gravity of Jade and Ruby Shall be Located within a Sphere of 2 cm of their Geometric Center**
14. **The CubeSat System Coordinate System Shall be Defined As Specified in Figure 1-1**
15. **The Local Coordinate System of Jade and Ruby Shall be Defined as Specified in Figure 1-1**
16. **The Ends of the Rails on the +Z/-Z Faces of the CubeSat System Shall have a Minimum Surface Area of 6.5 mm x 6.5 mm**
17. **The +Y/-Y Faces of Ruby and Jade Shall have a Length of 100 mm**
18. **Jade and Ruby Shall be Capable of Determining Relative Displacement between Each Other**
19. **The CubeSat System Shall be Capable of Recording Relative Displacement Data between Jade and Ruby**
20. **Low Friction, 2D Testing of the CubeSat System Release Mechanism Shall be Conducted**
21. **All Pressure Vessels Shall have a Factor of Safety of No Less Than 4**
22. **All CubeSat Components Shall be Rated to Operate within Temperature Range of at least -20⁰C to 70 ⁰C**
23. **Static Thrust Testing Shall be Performed with the Flight Version of All Pressure Vessels at a Pressure No Greater than 1x10-4 Torr Prior to CubeSat Integration**
24. **All Pressure Vessels Must Pass Thermal Cycle Testing between Temperatures of -30 ⁰C and 70 ⁰C for at Least Two Cycles or for 10 Hours**
25. **Low Friction, 2-D Dynamic Thrust Testing Shall be Conducted with All Pressure Vessels**
26. **The CubeSat System Must Survive Random Vibration Testing Relative to the NASA GEVS Qualification Profile**
27. **The CubeSat System Shall be Subjected to a Temperature of 60 ⁰C at a Pressure No Greater than 1x10-4 Torr for a Minimum of 6 Hours**
28. **The CubeSat System Shall be Able to Execute All Commands Associated with its Operation over RF**
29. **The CubeSat System Shall be Able to Close a Link with the SSRL Ground Station from a Distance of at least 200 meters**
30. **The CubeSat System Shall be able to Document the Functionality of Each of its Subsystems through the Running of a Full-Functional Test**

# Post-Launch Ejection Requirements

1. **The CubeSat System Shall not Broadcast in RF Until Ejection +45 Minutes**
2. **The CubeSat System Shall not Release Deployables Until Ejection +45 Minutes**
3. **The CubeSat System Shall Establish Communication Between Itself and the SSRL Ground Station**
4. **The CubeSat System Shall Pass a Health Check Administered from the SSRL Ground Station**

# Separation and Stabilization Requirements

1. **Jade and Ruby Shall be Capable of Separating from One Another with a Relative Velocity of No Greater than 5 cm/s**
2. **Jade and Ruby Shall Achieve a Local Slew Rate of Less than 1 deg/s**
3. **Jade and Ruby Shall Continuously Record Relative Displacement Data Between Each Other**

# Stationkeeping Requirements

# “Escape” Requirements

# Rendezvous Requirements