# Secondary STR Risk

* Previous skeleton design will not work
* Over/under allocation of mass for subsystems
* Select wrong components for STR subsystem

# Secondary COM Risk

* Wrong assumptions in link analysis.
* Preliminary component research takes too long

# Secondary PWR Risk

* Mistakes in Power budget assumptions
* Select wrong components for PWR Subsystem

# Secondary ADC Risk

* Mistakes in detumbling analysis
* Underestimated detumbling requirements
* Select wrong components for ADC subsystem
* Problems selecting GPS frequency

# Secondary CDH Risk

* Problems developing a functional block diagram for the S/C
* Software system overview takes too long